Another upgrade process

By samba

Download upgrade-last.tar file from server

sMS-200

sMS-1000SQ

Copy upgrade-last.tar to Eunhasu samba directory \\eunhasu\mw\data\music

Eunhasu page load like http://eunhasu/upgrade.php?upgrade_server=eunhasu/music&force=1

upgrade_server={EUNHASU_IP}/music is possible

By USB

Format USB to FAT32

Change USB label to SOTMDEBUG and it must upper case

Download upgrade-last.tar file from server

sMS-200

sMS-1000SQ

Copy downloaded upgrade-last.tar to the USB root directory

Make file named run_debug.txt in the USB

run_debug.txt file must contain following strings

upgrade force

By external utility

Refer Here