Requirement

sMS-200 V0.3.0 above or sMS-1000SQ Eunhasu V0.3.0 above

a Wifi dongle

a Wifi dongle which uses a RTL8812AU, RTL8812A, RTL8821A or RTL8814A chipset

Simple Instruction

Connect Wifi USB dongle into USB port. To setup Wifi feature on Eunhasu, the wired LAN should be connected.

Click 'Wifi' tab in System config page.

Click 'Wifi Router' button to show Wireless Access Point and it will take a few minutes to be detected the AP.

Select AP what you want.

Enter a password or secret if required.

Wait till the progress will be done.

After connecting successfully, you can see IP address like the screen shot below.

If you need remove Wifi connection information, Click 'Remove Wifi Information' button will remove all stored information include the name and password.

Eunhasu version >= V0.3.0 required. There might be connection error if you use wired and wireless network at the same time. Network speed could be degraded depends on wireless network status. After wireless connected, use IP address to connect

Reference

Video clip

Device IDs in driver

0x050D, 0x1106 : Belkin - sercomm

0x050D, 0x1109 : Belkin F9L1109 - SerComm

0x2001, 0x330E : D-Link - ALPHA

0x7392, 0xA822 : Edimax - Edimax

0x0DF6, 0x0074 : Sitecom - Edimax

0x04BB, 0x0952 : I-O DATA - Edimax

0x0789, 0x016E : Logitec - Edimax

0x0409, 0x0408 : NEC -

0x0B05, 0x17D2 : ASUS - Edimax

0x0E66, 0x0022 : HAWKING - Edimax

0x0586, 0x3426 : ZyXEL -

0x2001, 0x3313 : D-Link - ALPHA

0x1058, 0x0632 : WD - Cybertan*/

0x13B1, 0x003F : Linksys WUSB6300

0x1740, 0x0100 : EnGenius - EnGenius

0x2019, 0xAB30 : Planex - Abocom

0x07B8, 0x8812 : Abocom - Abocom

0x2001, 0x3315 : D-Link - Cameo

0x2001, 0x3316 : D-Link - Cameo

0x20F4, 0x805B : TRENDnet - Cameo

0x2357, 0x0101 : TP-Link - Archer T4U

0x2357, 0x0103 : TP-Link - T4UH

0x2357, 0x010D : TP-Link - Archer T4U AC1300

0x2357, 0x010F : TP-Link - Archer T4UHP

0x148F, 0x9097 : Amped Wireless ACA1

Last Updated: