Make the USB installation disk

Download the Eunhasu ISO image file

Eunhasu X86 V0.5.7

Eunhasu X86 V0.5.8

Eunhasu X86 V0.5.9

Eunhasu X86 V0.6.0

Download Rufus program

Download Rufus V3.4

Preparation

Prepare a 8GB(or above size) USB disk

Write in DD Image mode

Install Eunhasu OS to the sMB-Q370

Connect the USB disk to the USB port of the sMB-Q370

Connect a LCD monitor by a HDMI cable to the sMB-Q370

Connect a USB keyboard to the sMB-Q370 and turn on the PC

Hit a F7 button continuously while booting to go to booting disk selection windows

Select the USB disk and continue booting

Select the first string in Clonezilla windows

Clonezilla live with img Eunhasu-V0.5.5_sMB-Q370_60G_2023-11-29-01-img (VGA 800×600)

Select the installation disk

if your disk is M.2(NVME) Disk, select nvme0n1 or nvme0n2

if your disk is SATA Disk, select sda or sdb

Select Y or hit Enter if asked whether to continue installations

Once finished installations, reboot the PC

Expand Partition

Login to Eunhasu console

(ID: root / P/W: sotmaudio)

Once Logged in, enter "mc" to continue

Access to /root/install folder

if you use M.2(NVME) Disk, run setup_nvme.sh file.

if you use SATA Disk, run setup_sata.sh file.

Reboot the sMB-Q370 PC