Description

The sMS-1000SQ Windows Edition is the new way of music server based on Windows Server OS besides the original Linux OS based sMS-1000SQ.

Compared to Linux based music servers the diversified compatibility and the program support, the user friendly operation and such convenience functions have been attracted to ensure wide popularity of Windows OS based music servers. We found that Windows Server 2012 R2 based music servers further increased the level of sound quality.

After a longer period of reasearch and testing, SOtM proudly announce the first Windows OS based server which is simply so much better than any existing windows based server on the market, SOtM’s sMS-1000SQ Windows Edition is unequaled and capable to deliver the best sound quality available today.

Here are the key points why sMS-1000SQ Windows Edition is so special,

First, in order to fundamentally enhance the already great sound quality of a Windows Server 2012 R2 based music server, we chose to use the award-winning AudiophileOptimizer from Switzerland based Highend-AudioPC.

The AudiophileOptimizer is gaining popular favor from audiophiles around the world since more than two years. It is installed as first piece of software to ensure the best sound quality possible, even outperforming Linux based music servers. The Audiophile Optimizer specifically optimizes the Windows OS with only one goal in mind, to reproduce the highest sounds quality possible. In short, SOtM sMS-1000SQ Windows Edition is purified Windows OS by Audiophile Optimizer.

Second, the users can easily obtain high quality internet streaming service via ROON, and are capable to build the multi-zone network audio system configuration.

Third, Windows 8.1 OS can be installed as an option for those users desiring the common PC operation such as internet surfing, video playback and etc. With that, the sMS-1000SQ can be referred to Windows OS device, which is specialized in obtaining the high quality sound, allowing using of all functions on Windows OS based on the reputable sMS-1000SQ Hardware performance.

Fourth, sMs-1000SQ Windows Edition uses tX-USBexp as the basic feature and allows external power to the USB audio port presenting the highest sound quality.

Plus, the sMS-1000SQ Windows Edition allows using the internet streaming services like TIDAL or Qobuz, and common music playback programs like Foobar2000 and JRiver.

The sMS-1000SQ Windows Edition offers the best sound & technic as the original sMS-1000SQ does, both sMS-1000SQ series provide the most satisfied sound quality no matter what kinds of audio systems users may desire to build, they can enjoy fantastic sound performance with SOtM sMS-1000SQ server.

Specification

OS

Windows Server 2012 R2 or Windows 8.1

Available audio playback software

Roon

TIDAL

Qubuz

Foobar2000

JRiver

PowerDVD

Etc.

Basic standard Storage

32G SSD for Windows Server 2012 R2

250G SSD for Windows 8.1 OS

Optional data storage

max.4TB HDD or max.2TB SSD

USB output model

Audio grade USB 3.0 port (tX-USBexp)

External power input jack

USB power on/off switch

USB audio class 2.0 support

Support format : 32bit/384KHz PCM, DSD

Digital output model

AES/EBU, Coaxial, Optical output

Support format : 24bit/192KHz PCM

Analog output model

Balanced,Unbalanced output

Balanced output voltage : 1.9Vrms

Unbalanced output voltage : 0.95 Vrms

Support format : 32bit/192KHz PCM

THD+N : 0.005% > @ 1KHz

Output band width : -3dB@100KHz

Power requirement

Input Voltage : +19Vdc

Power : Max 60W

Operating environment

Operating temperature : +10 ~ +30℃

Storage temperature : 0 ~ +40℃

Operating & storage humidity : 10% ~ 90%

Dimension

360×68×240(mm)

Weight

4Kg >