tX-USB hub

Precaution

Please read this instruction carefully before use.

Do not attempt to disassemble or modify the product.

Keep the product away from the external shocks or vibrations.

Do not use the damaged or peeled cables.

Do not use the unit outdoors.

Product specifications and features are subject to change without notice.

Supplied components

tX-USBhubEX Unit

Operating instruction

Specification

USB host interface port

USB 2.0 Type B connector

USB output Port

Type A USB 2.0 connector x 2

USB port power on/off switch x 2

USB interface chip set

USB 2.0 Compliant HUB controller

HS(480 Mbps), FS(12 Mbps), LS(1.5 Mbps) support

Power input

Input voltage : +6.5V ~ +9Vdc

Input current : 2A max

5.5mm OD, 2.1mm ID adaptor jack

USB port output power

Output voltage : +5.0V(+0.5V, -0.25V)

Over current protect : 0.8A at 20°C

Recommend output current : 0.5A >

Operating environment

Operating temperature : +10 ~ +30℃

Storage temperature : 0 ~ +40℃

Operating & storage humidity : 10% ~ 90%

Product Outline

USB output port no. 1 : Connect to USB audio device.

Power switch of USB output port no. 1 : Switch ON, if the connected USB audio device requires USB power. If not, switch OFF.

USB output port no. 2 : Connect to USB audio device.

Power switch of USB output port no.2 : Switch ON, if the connected USB audio device requires USB power. If not, switch OFF.

Power input jack : The power, 6.5Vdc ~ 9Vdc, 2A, is required to operate the unit. (jack size : 5.5mm OD, 2.1mm ID) A supplied 9V/2A adopter, mBPS-d2s or sPS-1000 can be used.

USB input port : Connect to an USB port of your PC or server by USB cable (Type A - to - Type B).

Recommend using one of USB ports only. If you use both USB ports at the same time, sound quality may degrade.

Product user guide

tX-USBhubEX is 2 ports USB2.0 external hub designed for the best USB audio performance.

Put the unit on a proper place, and connect to an USB port of PC or server by USB cable (Type A - to - Type B)

Connect the supplied 9Vdc, 2A power wall adopter, mBPS-d2s or sPS-1000 power supply to the power input jack to operate the unit.

And then the green LED of the unit will be lit on and automatically recognized as a USB hub without additional driver installation.

If the connected USB audio device requires +5V, switch ON the power switch, if not, switch OFF.

Connect one of USB output ports to USB Audio device by USB cable(Type A - to - Type B)

Warranty Information

Free warranty service

In case of the defect is found caused by the design or the production flaw while using the device properly, a manufacturer is responsible for the faulty product and the free warranty service for 1 year from the date of purchasing.

Even in the warranty service period, malfunction or damage of products caused by the inevitable incident such as a natural disaster is not subject of the free warranty service.

Warranty service at a cost

The product that free warranty service period is expired.

Malfunction of the product caused by a user’s fault.

Malfunction of the product caused by incidents.

Malfunction of the product caused by a natural disaster such as earthquake, flood, lightning & etc.

In case of the warranty service at a cost, a customer should cover the transportation costs.

Samples of a user’s fault

In case of attempts to disassemble or modify the device

In case of not following the instructions on this manual

Please read this operating instructions & Q&A board on our website carefully before asking for the warranty service.