MPD / DLNA renderer

MPD is a high performance music playback service that can play music files on a USB storage device or network share folder. Eunhasu has only DLNA audio renderer not include other DLNA stack. You can use Eunhasu with a DLNA server. However, sMS-1000SQ Eunhasu product has a DLNA server feature which is MinimServer. You could use 'MPD / DLNA renderer' with MinimServer if you have sMS-1000SQ Eunhasu.

Name: A name of Eunhasu's MPD & DLNA appearing on MPD controlling App and DLNA controlling App. This can be changed if you need.

Audio device config: Select a radio button of USB DAC which is going to use and click 'Save changes' to use the USB DAC.

DOP enable: Check for using DOP function while playing DSD music file.

Native DSD type 0: To use 8-bit DSD_U8 format DAC. (e.g. BeagleBone Black using Botic driver)

Native DSD type 2: To use 32-bit DSD_U32_BE format DAC. (e.g. XMOS-based USB DACs or Marantz/Kenwood DAC)

Replay gain: Choose Replay gain among None, Album or Track.

OpenHome DLNA Renderer: Check for using OpenHome DLNA Renderer feature.

Library auto update: Check for auto-scanning and updating the library.

Native DSD feature is available from Eunhasu V0.3.2.

MPD clients

MPDroid: https://play.google.com/store/apps/details?id=com.namelessdev.mpdroid

M.A.L.P. - MPD Client: https://play.google.com/store/apps/details?id=org.gateshipone.malp

MPod: https://itunes.apple.com/kr/app/mpod/id285063020?mt=8 out of dated

MPDluxe: https://itunes.apple.com/us/app/mpdluxe/id991758069?mt=8

Gnome Music Player Client: https://gmpclient.org/installation

Chimney: https://www.microsoft.com/en-us/store/p/chimney/9wzdncrfj6jx

Reference: http://mpd.wikia.com/wiki/Clients

how to connect and access NAS in sMS-200

How to connect NAS to Squeezelite or MPD/DLNA on sMS-200

Last Updated: